Meet the BLACKBOLT BA20: a universal motorized 360 degrees mounting kit. Connect your camera to the kit and enjoy the professional precision of motorized movements. The BA20 can be connected to every camera with a ¼” tripod screw and rotates and moves in different directions.

There are 3 different types of rotating:
Continu rotation, left or right, 360°.
Swing, 60° left and 60° right = 120° total.
Stop & go, 360° turn with a short stop on every 90°.

In 3 different types of speed:
Timelaps, 360° turn in 60 minutes
Normal, 360° turn in 40 seconds
Fast, 360° turn in 25 seconds

The Blackbolt BA20 kit is included with a BA10 suction cup. The BA10 can be easily attached on flat and curved surfaces. The suction cup and its patented high-resilience sticky pads are twice more powerful than standard pads. It can swing a 15lb bowling ball, but also resist the vibrations happening during high speed action.

 Watch this movie: <https://www.youtube.com/watch?v=Bx1EmgoXWL4> to see what the Blackbolt is capable of.